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Consale

Speed Grade: -

Minimum period: 3.934ns (Maximum Frequency: 254.184MHz)

Minimum input arrival time before cloc)

2.625n2

Maximum output required time after clock: 7.704ns
Maximum combinational path delay: 8.796ns

Brocess "Synthesize - XST" completed successfully

_
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