工程文件
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程序文件
[image: image2.png]input clk_50M,
input reset,

output reg [7:0]HEX1,
output reg [7:0]HEX2

always@ (posedge clk 50M or posedge reset)
if (reset)
count<=32"d0;
else
if (count>=49 999 999)
count<=327d0;
else
count<=count+32'd1; // =

reg [4:0] time cnt=5'd24;/ /2
always@ (posedge clk 50M or posedge reset)
if (reset)

time_cnt<=5'd24;

else
ifflcount>=19 999 999
if (time_cnt==5'd0)
time_cnt<=5'd0;

BES
time_cnt<=time_cnt-5'dl;

else
time_cnt<=time_cnt;




程序编译
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RllType  ID  Message

» A 13024 output pins are stuck at VCC or GND
(286030 Timing-Driven Synthesis is running
» @ 16010 Generating hard block partition "hard block:auto_generated_inst"
» @ 21057 Implemented 121 device resources after synthesis - the final resource count might be different
gl @ Quartus II 64-Bit Analysis & Synthesis was successful. 0 errors, 6 warnings
B -





Testbench
[image: image4.png]“timescale 1 ns/ 1 ns
module timer vlg_tst():

reg clk_50M;
reg reset;

)

HEX1 (HEX1),
-HEX2 (HEX2) ,
.clk _50M(clk_50M),
.reset (resdft)

c1k_50M=0;
4107
c1k_50M=1;





仿真图
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