工程文件
[image: image1.png]| car_LED.cache

. car LED.hw

(b car_LED.ip_user files.

1 car LED.runs.

b car_LED.sim

1 car LED.sres

. car LEDxpr

] test fenping_behavwcfg
] vivadojou

] vivadolog

] vivado 7392 backupjou
] vivado_7392.backuplog
] vivado_8068.backupjou
] vivado_8068.backuplog
] vivado_pidg06B.str

2020/6/18 23:02
2020/6/18 23:02
2020/6/18 22:50
2020/6/18 23:02
2020/6/18 23:02
2020/6/18 23:02
2020/6/18 23:14
2020/6/18 23:18
2020/6/18 23:18
2020/6/18 23:18
2020/6/17 0:14

2020/6/17 0:16

2020/6/18 22:47
2020/6/18 22:47
2020/6/18 21:45

iz
P

B

B

B

B

Vivado Project Fi
WCFG #

JoU Stk

wrifle

JoU Stk

wrifle

JoU Stk

wrifle

STR 32t

7x8
3k8
2x8
15K8
2x8
3k8
2x8
5K8
129k8




程序文件
[image: image2.png]| 3 X | P
Flow Tavigator «

4 Project Mamsger
B Project Settines

6% haa Sources
Lengusge Template:

TF 17 catalos

TP Integrator
¥ create Block Desi(
pen Block Design

Generste Elock De

4 Similation
B simiation Settin
@ Ren Simadation

4 BIL tndlysic
B ELaboration Settiy
5% Open Flaborated D

Synthesis
B Synthesis Setting
® Run Symthesis

& Open Synthesized |

Inglenentation
& Inplamentation S
Run Tnplenentatio

52 Open Tnplenented |

Progran and Debug
B Bitstrenn Setting
Genarate Bitstrem

&Y Open Hordware Man

G % 3 (55 Default Layout =

Project Nemager — car 1ED
Sourcas _oex
AaTE e 3|
S D Design Sowrees
- Constraints
) Simalation Sources
Hierarchy| Librariss |Congile Order

& Sources | 7 Tamplates
Sourcs Fils Fropertiss _oex

@ car 1ED.v

Loeation: F:/VIVADO_progran/BASTS3_pro/car_LED 1

Type Veritog | [

Library il aefeiiin | ()

G 21m

Wodified: Todey at 22:23:53 P

Copied to: F:/VIVADO_progran/BASTS3_pro/ car_LED_T043/¢
Resborly Mo

Genersl | Propertias

Design Runs
A rane Constraints
RV constes_1
: £ impl_t constrs_1

Synthesis and Inplementation Out-

F/VIVADO pr

Project Sumary X

5 car_LED.v X

ogran/BASTS3_prof car_LED_T03/ car_LED_sin/car LED. srcs/sources_1/new/ car LED v

clk_100M,
right_key,

right LED,
left LED,
[1:0] brake_LED

Status
Synthesis Out-of-date
Inplenentation Out-of

WIS IS WS TS TIPS Failed Restes LU FE BRMI URMN  DSP  Start Elapsed  Strategy
2 @ 5/18/: i 29 Vivado Synthesis Defaults (ivado Synthesis
-date CIETI") 0 0 6/18/20 10:48 P 00:01:07 Vivade Inplementation Defaults (Vivado Inplemes





[image: image3.png]Q=== R
S desicn Sowrees O
XY
@ i_fenping - fenping (fenping v)
@ i_brake_ctrl - brake_ctrl (brake ctrl v)
@ constraints ()
SSimdation Seurees )





管脚约束文件
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